Coolant On for all Tools

Tool # :                43
Type:                   Insert End Mill (Preferred) or Solid Carbide
Diameter:               .750"
Corner Type:            Radius .125"
Flutes:                 3 
Minimum Flute Length:   .150" 
Minimum Exposed Length: .6" 

Tool # :                18
Type:                   End Mill, Carbide
Diameter:               .75"
Corner Type:            Square (Or any Radius (Used for periphery cut))
Flutes:                 3 
Minimum Flute Length:   1.250" 
Minimum Exposed Length: 1.300" 

Tool # :                4
Type:                   Ball Nose, Carbide
Diameter:               .5"
Flutes:                 2 
Minimum Flute Length:   .25" 
Minimum Exposed Length: .6" 

Tool # :                8
Type:                   End Mill, Carbide
Diameter:               .375"
Corner Type:            Square
Flutes:                 3 
Minimum Flute Length:   .375" 
Minimum Exposed Length: .6" 

Tool # :                5
Type:                   Ball Nose, Carbide
Diameter:               .125"
Flutes:                 2 
Minimum Flute Length:   .125" 
Minimum Exposed Length: .6" 

Tool # :                21
Type:                   End Mill, Carbide
Diameter:               .0938"
Corner Type:            Square
Flutes:                 4 
Minimum Flute Length:   .375" 
Minimum Exposed Length: .7" 

Tool # :                23
Type:                   Spot Drill, 90deg, HSS
Diameter:               .5"
Flutes:                 2 
Minimum Flute Length:   .25" 
Minimum Exposed Length: .75"

Tool # :                22
Type:                   Drill, HSS or Carbide
Diameter:               .242" (Letter "C")
Flutes:                 2 
Minimum Flute Length:   .75" 
Minimum Exposed Length: 1.5"

Tool # :                24
Type:                   Reamer, HSS
Diameter:               .2495"  
Minimum Flute Length:   .5" 
Minimum Exposed Length: 1.5"

Tool # :                25
Type:                   Reamer, HSS
Diameter:               .2502"
Minimum Flute Length:   .5" 
Minimum Exposed Length: 1.5"